

Figure : TPS Switch #5, 12 Ohm load




Figure : TPS Switch #5, no load




Figure : Switch #4 with 10 nF instead of 3.9 nF C\_TIMER. Steady-state IMON = 0.085 V




Figure : TPS switch, 12 Ohm load, steady stae IMON = 0.002 V, C\_TIMER = 0.1 uF




Figure : PPT Switch w/ 10 nF cap on C\_TIMER, Load = 12 Ohm